## Description

Windows NT 4.0 allows remote attackers to cause a denial of service (crash) via extra source routing data such as (1) a Routing Information Field (RIF) field with a hop count greater than 7, or (2) a list containing duplicate Token Ring IDs.

## Severity

Overall Severity: N/A

### CVSS Metrics

Type | Score | Severity | Vector
--- | --- | --- | ---

## Affected Products

### microsoft - windows_nt

Affected Versions:

- 4.0

## References

- http://marc.info/?l=bugtraq&m=90763508011966&w=2
- http://marc.info/?l=ntbugtraq&m=90760603030452&w=2
- http://support.microsoft.com/support/kb/articles/Q179/1/57.asp
  Patch Vendor Advisory
- http://www.iss.net/security_center/static/1399.php
- http://marc.info/?l=bugtraq&m=90763508011966&w=2
- http://marc.info/?l=ntbugtraq&m=90760603030452&w=2
- http://support.microsoft.com/support/kb/articles/Q179/1/57.asp
  Patch Vendor Advisory
- http://www.iss.net/security_center/static/1399.php

Neural Processor Active