## Description

Multiple buffer overflows in ISC DHCP Distribution server (dhcpd) 1.0 and 2.0 allow a remote attacker to cause a denial of service (crash) and possibly execute arbitrary commands via long options.

## Severity

Overall Severity: N/A

### CVSS Metrics

Type | Score | Severity | Vector
--- | --- | --- | ---

## Affected Products

### isc - dhcp_client

Affected Versions:

- 1.0

### isc - dhcp_client

Affected Versions:

- 2.0

## References

- ftp://ftp.isc.org/isc/dhcp/dhcp-1.0-history/dhcp-1.0.0-1.0pl1.diff.gz
  Patch
- http://ciac.llnl.gov/ciac/bulletins/i-053.shtml
  Patch Vendor Advisory
- http://marc.info/?l=bugtraq&m=90221101925960&w=2
- ftp://ftp.isc.org/isc/dhcp/dhcp-1.0-history/dhcp-1.0.0-1.0pl1.diff.gz
  Patch
- http://ciac.llnl.gov/ciac/bulletins/i-053.shtml
  Patch Vendor Advisory
- http://marc.info/?l=bugtraq&m=90221101925960&w=2

Neural Processor Active