## Description

Windows 95 and Windows 98 systems, when configured with multiple TCP/IP stacks bound to the same MAC address, allow remote attackers to cause a denial of service (traffic amplification) via a certain ICMP echo (ping) packet, which causes all stacks to send a ping response, aka TCP Chorusing.

## Severity

Overall Severity: N/A

### CVSS Metrics

Type | Score | Severity | Vector
--- | --- | --- | ---

## Affected Products

### microsoft - windows_95

Affected Versions:

- *

### microsoft - windows_98

Affected Versions:

- *

## References

- http://marc.info/?l=ntbugtraq&m=91849617221319&w=2
- http://www.securityfocus.com/bid/225
- https://exchange.xforce.ibmcloud.com/vulnerabilities/7542
- http://marc.info/?l=ntbugtraq&m=91849617221319&w=2
- http://www.securityfocus.com/bid/225
- https://exchange.xforce.ibmcloud.com/vulnerabilities/7542

Neural Processor Active