## Description

The PMTU discovery procedure used by HP-UX 10.30 and 11.00 for determining the optimum MTU generates large amounts of traffic in response to small packets, allowing remote attackers to cause the system to be used as a packet amplifier.

## Severity

Overall Severity: N/A

### CVSS Metrics

Type | Score | Severity | Vector
--- | --- | --- | ---

## Affected Products

### hp - hp-ux

Affected Versions:

- 10.30

### hp - hp-ux

Affected Versions:

- 11.00

## References

- http://www.securityfocus.com/bid/944
- http://www.securityfocus.com/templates/advisory.html?id=2041
- http://www.securityfocus.com/bid/944
- http://www.securityfocus.com/templates/advisory.html?id=2041

Neural Processor Active