## Description

Buffer overflow in hybrid-6 IRC server commonly used on EFnet allows remote attackers to execute commands via m_invite invite option.

## Severity

Overall Severity: N/A

### CVSS Metrics

Type | Score | Severity | Vector
--- | --- | --- | ---

## Affected Products

### hybrid_network - hybrid_ircd

Affected Versions:

- *

### hybrid_network - hybrid_ircd

Affected Versions:

- 5.03p7

## References

- http://www.efnet.org/archive/servers/hybrid/ChangeLog
- http://www.securityfocus.com/bid/581
- http://www.efnet.org/archive/servers/hybrid/ChangeLog
- http://www.securityfocus.com/bid/581

Neural Processor Active