## Description

3Com HiPer Access Router Card (HiperARC) 4.0 through 4.2.29 allows remote attackers to cause a denial of service (reboot) via a flood of IAC packets to the telnet port.

## Severity

Overall Severity: N/A

### CVSS Metrics

Type | Score | Severity | Vector
--- | --- | --- | ---

## Affected Products

### 3com - hiperarc

Affected Versions:

- *

## References

- http://marc.info/?l=bugtraq&m=93458364903256&w=2
- http://marc.info/?l=bugtraq&m=93492615408725&w=2
- http://www.osvdb.org/6057
- http://marc.info/?l=bugtraq&m=93458364903256&w=2
- http://marc.info/?l=bugtraq&m=93492615408725&w=2
- http://www.osvdb.org/6057

Neural Processor Active