## Description

Cabletron SmartSwitch Router (SSR) 8000 firmware 2.x can only handle 200 ARP requests per second allowing a denial of service attack to succeed with a flood of ARP requests exceeding that limit.

## Severity

Overall Severity: N/A

### CVSS Metrics

Type | Score | Severity | Vector
--- | --- | --- | ---

## Affected Products

### cabletron - smartswitch_router_8000_firmware

Affected Versions:

- 2.0

## References

- http://razor.bindview.com/publish/advisories/adv_Cabletron.html
  Patch Vendor Advisory
- http://www.securityfocus.com/bid/821
- http://razor.bindview.com/publish/advisories/adv_Cabletron.html
  Patch Vendor Advisory
- http://www.securityfocus.com/bid/821

Neural Processor Active