## Description

Buffer overflow in POP servers based on BSD/Qualcomm's qpopper allows remote attackers to gain root access using a long PASS command.

## Severity

Overall Severity: CRITICAL

### CVSS Metrics

Type | Score | Severity | Vector
--- | --- | --- | ---
CVSS v3.1 | 9.8 | CRITICAL | `CVSS:3.1/AV:N/AC:L/PR:N/UI:N/S:U/C:H/I:H/A:H`

## Affected Products

### qualcomm - qpopper

Affected Versions:

- 2.4

## References

- ftp://patches.sgi.com/support/free/security/advisories/19980801-01-I
- http://www.securityfocus.com/bid/133
- ftp://patches.sgi.com/support/free/security/advisories/19980801-01-I
- http://www.securityfocus.com/bid/133

Neural Processor Active